TOP-228WF- Hot point function

1. Keep the camera is with power “12V” for 1 minute at least

2.Find the wife which named “GW-IPC” in mobile and connect (the WIFI is from camera and password is empty )

1. Open the soft in mobile and watch the video

NOTICE:IF U HAVE USED THE CAMERA BY P2P OR IN THE SAME INTERNET OR OTHER WAY (IT MEANS YOUR PHONE HAS EVER USED WITH THIS CAMERA IN ANYWAY ), WHEN U HAVE PRESS THE “RESET ” BUTTON BUT CAN’T FIND THE CAMERA’S WIFI ,PLEASE OPEN THE SOFT ,MAYBE YOUR PHONE HAS CONNCET THE WIFI ALREADY